
[newcurve]
cockpit_tacholinie

[pnt]
0
0
[pnt]
5
8
[pnt]
10
15
[pnt]
20
28
[pnt]
30
50
[pnt]
40
73
[pnt]
50
95
[pnt]
60
118
[pnt]
70
127
[pnt]
80
140
[pnt]
90
187
[pnt]
100
210
[pnt]
110
215
[pnt]
120
257

[newcurve]
cockpit_oeldruck

[pnt]
300
23

[pnt]
400
29

[pnt]
600
46

[pnt]
800
61

[pnt]
1000
71

[newcurve]
odometer_10er-uebertrag
[pnt]
0
0
[pnt]
0.9
0
[pnt]
1
1

[newcurve]
cockpit_engine_temperature

[pnt]
40
0

[pnt]
60
12

[pnt]
80
26

[pnt]
100
44

[pnt]
120
60

[newcurve]
motortuer_mehamizm_rot

[pnt]
0
0

[pnt]
0.2
6

[pnt]
0.4
12

[pnt]
0.6
17.5

[pnt]
0.8
21

[pnt]
1
22.5

[newcurve]
motortuer_mehamizm_trans

[pnt]
0
0

[pnt]
0.2
0

[pnt]
0.4
0.02

[pnt]
0.6
0.06

[pnt]
0.8
0.11

[pnt]
1
0.16

[newcurve]
podsvet_prib_light

[pnt]
0
0

[pnt]
1
1

[const]
automatic_battery_switch
0

[const]
auxheat_via_button
1

[const]
wiper_lever
0

[newcurve]
cockpit_warndruck

[pnt]
550000
1

[pnt]
700000
0

[const]
cockpit_gangwahltaster_alt
0

[const]
cockpit_zentralschmierung_dist
50

[const]
cockpit_zentralschmierung_maxtime
30

[const]
cockpit_gear_D_only
0

[const]
cockpit_has_20h_switch
0

[const]
cockpit_has_retarderswitch
1

[const]
cockpit_has_coolingswitch
1

[const]
cp_fahrertuer_anschlagseite
1

[const]
cockpit_aftdoorlight_condition_D92
0



=============================================
Inverse Widerstände (Leitwerte) in 1/Ohm.


Allgemeiner Stromverbrauch Panel (sonstige): 1x40W (1x0.0174 1/Ohm)

[const]
cp_general_Rinv
0.0174

.............................

Frontheizgerät: 1x60W (1x0.104 1/Ohm)

[const]
cp_klimator_Rinv
0.104

.............................

Hintere Heizgeräte (zusammen): 60W (0.104 1/Ohm)

[const]
cp_cabinheater_Rinv
0.104

.............................

[const]
Matrix_Waittime
0.5

[const]
Matrix_Changetime_Terminus
1.83

[const]
Matrix_Changetime_Nr
1.25
